PL2260+
Ver 1.5.0.2
1. The 'Auto Repeat' feature dexribed in 1.5.0.1 #2 below is furthee expanded to include 'Blank Chk' and Illegal Bit' tests.
2. When using either of the 'CRC32' buttons in the 'More Panel', when the CRC32 figure is obtained a search is automatically initiated for a match against the CRC32 tables. Eliminates the need to also have to click the 'CRC32 Srch' button.
3. Similarly, when typing or copying a CRC32 figure into the CRC32B text field, use of the keyboard 'Enter' key will initiate the search.

Ver 1.5.0.1

Changes In the 'More Panel':
1. Previously when doing an 'Input File' of an Absolute Binary formatted file, a field would display the calculated Sumcheck of the data which can be used to compare with the Sumcheck reported by the programmer to detect possible transfer errors. This feature has now been expanded to provide the calculated Sumcheck of most any formatted file.
2. The 'Auto Repeat' feature for the 'PROGRAM' operation now expanded to include repeated operation related to the 'Verify Dev' button. 

Changes in the 'Extras Panel'
3. The 'Translate Files' feature now includes conversion of Octal Hex formatted files. (Data IO codes 30-38).
4. The 'Auto Poll' (or auto connect) feature now more functional for non-UniFamily models.
5. Previously, the 'Chk File IO Format' feature might report the format of an Intel 'MCS-86' or '32-Bit' file as the lower capacity 'Intellec 8/MDS' file.

Other:
6. Previously when closing PL2260+, the serial port of the computer (if had been in use) would sometimes remain open preventing other apps from using it.